{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":4},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":9,"rows_kept":5,"merged":[[0,0,0,8]]}
["直饮水机设备报价明细"]
["设备名称","设备照片","设备具体参数","维修维保情况","直饮水/废水比例","更换滤芯频率","是否包含上下水管路铺设","附加优惠条件","租赁费用/年单价及税点"]
["客用直饮水机",null,"1、直饮水机供水量：满足50人以上；\n2、过滤模式应为先进的反渗透过滤模式；\n3、直饮水机需有必要净水箱杀菌技术；\n4、需提供常温水、开水两种种出水方式；\n5、必须有中温水（40-50℃）出水模式；\n6、净水箱不低于15L（或者供水量）\n7、额定电压：220v/50Hz，额定功率：不超过3000（含）W。\n8、外观尺寸范围(上下百分之十之内)：500*500*1500mm","1、必须有水质自动检测系统，滤芯更换要求一次性全换，不接受分级更换；\n2、要求有厂家或代理商的自营售后，不接受外包服务；\n3、设备移机，应提供免费的移机服务；\n4、设备形象，为保证直饮水机的外观形象要求有更换整机或者外壳的服务"]
["服务台台式（墙上）直饮水机",null,"1、直饮水机供水量：满足30人以上；\n2、过滤模式应为先进的反渗透过滤模式；\n3、直饮水机需有必要净水箱杀菌技术；\n4、需提供常温水、开水两种种出水方式；\n5、额定电压：220v/50Hz，额定功率：不超过600（含）W。\n6、外观尺寸范围(上下百分之十之内)：300*300*500mm\n7、安装方式：壁挂、台座放","1、必须有水质自动检测系统，滤芯更换要求一次性全换，不接受分级更换；\n2、要求有厂家或代理商的自营售后，不接受外包服务；\n3、设备移机，应提供免费的移机服务；\n5、设备形象，为保证直饮水机的外观形象要求有更换整机或者外壳的服务"]
["员工用直饮水机",null,"1、直饮水机供水量：满足200-300人；\n2、过滤模式应为先进的反渗透过滤模式；\n3、直饮水机需有必要净水箱杀菌技术；\n4、需提供常温水、开水两种种出水方式；\n5、净水箱不低于60L（或者供水量）；\n6、额定电压：220v/50Hz，额定功率：不超过3000（含）W。\n7、外观尺寸范围(上下百分之十之内)：800*800*1800mm；","1、必须有水质自动检测系统，滤芯更换要求一次性全换，不接受分级更换；\n2、要求有厂家或代理商的自营售后，不接受外包服务；\n3、设备移机，应提供免费的移机服务；\n4、设备形象，为保证直饮水机的外观形象要求有更换整机或者外壳的服务"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}