{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["防盗系统"],"not_rendered":{"images":34},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"防盗系统","index":0,"n_rows":43,"n_cols":12,"rows_kept":43,"merged":[[0,0,0,11],[39,0,39,11],[40,0,40,4],[40,5,40,11],[41,0,41,4],[41,6,41,7],[41,8,41,11],[42,0,42,4],[42,6,42,11]],"flags":["formulas_cached_only"]}
["北国超市防损系统招标清单："]
["序号","图片","名称","品牌","型号","参数","材质/颜色","使用范围","单位","单价/元","保修期限","交货周期"]
[1,null,"声磁防盗系统天线",null,null,"双支座软标签检测范围宽达1.6m，          尺寸：高153*宽41.5*厚13CM，输入电压：100-240V,最大功耗：100W,最大电流：450MA,工作频率：58KHz。 ","ABS/灰色","收银通道或者出入口安装"]
[2,null,"声磁亚克力防盗系统天线",null,null,"双支座软标签检测范围宽达1.6m，          尺寸：高156*宽41.5*厚13CM，输入电压：100-240V,最大功耗：100W,最大电流：450MA,工作频率：58KHz。 ","透明亚克力","收银通道或者出入口安装"]
[3,null,"地埋式声磁系统",null,null,"软标检测距离地板以上0.8-1.2米，硬标1.3-1.6米，高156*宽41.5*厚13CM，输入电压：100-240V,最大功耗：100W,最大电流：450MA,工作频率：58KHz。","ABS/灰色","地埋安装"]
[4,null,"声磁软标签消磁器  ",null,null,"软标签消磁距离达到12cm","ABS/黑灰色","收银台安装，消磁软标签"]
[5,null,"消磁桶+控制器",null,null,"长*宽*高525*400*500mm  容积37L   ","ABS/灰色","自助收银台安装，消磁软标签"]
[6,null,"强磁取钉器",null,null,"磁力达到14000GS","外观铝合金","解锁超强磁力硬标签和功能标签"]
[7,null,"声磁硬标签（超强磁、防屏蔽）",null,null,"66.5*16.5*19mm","ABS/乳白","用专用钉子钉到商品上保护商品"]
[8,null,"声磁高性能软标签",null,null,"44.8*10.3*1.9","条码、白、黑","一次性防盗标签，粘贴于商品，可消磁"]
[9,null,"声磁标准高品质软标签",null,null,"44.5*11.1*2","条码、白、黑","一次性防盗标签，粘贴于商品，可消磁"]
[10,null,"声磁冷冻标签",null,null,"45*11*2","红色、条码、白","一次性防盗标签，粘贴于商品，可消磁"]
[11,null,"声磁水标",null,null,"44.7*11.3*3","条码、白","一次性防盗标签，粘贴于商品，可消磁"]
[12,null,"高品质酒瓶签",null,null,"直径50mm，绳长160mm","灰白色","可保护白酒、油、锅、厨具、剪刀等"]
[13,null,"高端声磁酒瓶扣  ",null,null,"内缩式绑带","灰白色","防止顾客拿酒瓶时带倒旁边的酒瓶"]
[14,null,"防偷喝酒瓶帽",null,null,"85mm*67mm","灰白色","保护高端红酒，可防止偷喝"]
[15,null,"高品质奶粉签",null,null,"直径50mm，绳长480mm","灰白色","可保护桶装奶粉，小号可保护咖啡"]
[16,null,"奶粉底托 标准",null,null,"(大) Ø150mmX33mm","ABS/灰白","保护标准桶装奶粉"]
[17,null,"奶粉底托 小桶",null,null,"(小) Ø122mmX33mm","ABS/灰白","保护小桶装奶粉"]
[18,null,"挂钩标签",null,null,"55.1*54*22.4","ABS/灰白","可保护塑封的商品，同时方便挂到挂钩"]
[19,null,"袋装商品保护夹",null,null,"69*42*16mm","黑色/灰色","可保护塑料袋包装的商品"]
[20,null,"保温杯防盗扣",null,null,"带长320mm","ABS/灰白","保护各种保温杯及水杯"]
[21,null,"带绳硬标签（远距离）",null,null,"50*12*20（绳长175)","灰白色","挂到需要保护的商品上"]
[22,null,"钢丝绳",null,null,"175mm","白色/黑色","与硬标签一起使用。"]
[23,null,"硬标签专用钉",null,null,"19mm","不锈钢","与硬标签一起使用。"]
[24,null,"牙膏防掉包保护盒 大",null,null,"55*45*(205~235)","高品质材料、通透、高抗压抗冲击、不易老化","保护牙膏，防止掉包。"]
[25,null,"牙膏防掉包保护盒 小",null,null,"48*39*(185~215)","高品质材料、通透、高抗压抗冲击、不易老化","保护牙膏，防止掉包。"]
[26,null,"蜘蛛标签",null,null,"57Dia*47mm","黑色/灰色","保护贵重的商品，带自鸣功能"]
[27,null,"剃须刀保护盒",null,null,"内部尺寸：高220mm*宽116.5mm*厚65mm","高品质材料、通透、高抗压抗冲击、不易老化","保护电动剃须刀、化妆品"]
[28,null,"化妆品保护盒",null,null,"内部尺寸：高170mm*宽136mm*厚60mm","高品质材料、通透、高抗压抗冲击、不易老化","保护化妆品"]
[29,null,"超大保护盒",null,null,"内部尺寸：高200mm*宽150mm*厚50mm","高品质材料、通透、高抗压抗冲击、不易老化","可将不易用标签保护且贵重的商品装到盒子里保护。"]
[30,null,"多功能保护盒 ",null,null,"内部尺寸：高150.5mm*宽118.5mm*厚45mm","高品质材料、通透、高抗压抗冲击、不易老化","可将不易用标签保护且贵重的商品装到盒子里保护。"]
[31,null,"电池保护盒 ",null,null,"内部尺寸：高79mm*110mm*32mm ","高品质材料、通透、高抗压抗冲击、不易老化","保护单排或双排电池"]
[32,null,"方形雷达自动感应门",null,null,"尺寸：L2400*W2100*H1170 ","镜面不锈钢，表面镀铬","入口安装，带计数器，反推报警"]
[33,null,"防盗购物袋",null,null,"尺寸：50*40*10cm","进口韩国防雨布料","入口封包用"]
[34,null,"声磁防盗天线架子",null,null,"高153*宽41.5*厚13CM","ABS/灰色","收银通道或者出入口安装"]
[35,null,"防盗天线主板或电源板维修"]
[36,null,"防盗天线更换主板维修"]
[37,null,"天线移机"]
["注：1、以上报价含税（增值税专用发票    %）、含运费；\n    2、保修期限从客户签收产品当日起开始核算；\n    3、交货周期从合同签订、收到首付款当日起核算。"]
["供货企业名称：",{"$nulls":4},"办公地址："]
["电话：            传真：",{"$nulls":4},"联系人：","电话：",null,"安装周期：   "]
["开户行：  ",{"$nulls":4},"账号：","付款方式：合同约定。"]